

HGXL Airflow Sleeve Removal

Unit E2

Fairoaks Airport

Chobham

Woking

Surrey

GU24 8HU

Tel: 01276 859443

*VAT registered: 833886490*

*Hayden Krause*

Date: 29/11/2017

* Open the HGXL Door and remove both sensors from the side wall. The connectors have a sheath. Pull on the knurled section of the connectors as shown.





* Remove the metal tube



* Remove the two button heat screws using 2.5mm hex key (bottom right and top left).



* Carefully remove airflow sleeve



* Access to the cross head screws for removal and re-seating



**NOTE: Be extra careful when placing the airflow sleeve back into position. The fin features are delicate.**



Fins

**NOTE: When re-positioning sensors the red dot on the connectors should be facing towards the product door.**